IFC building model
Schema: "IFC2X3"
File name: "Sample.ifc"
Time stamp: "12/11/2021 2:51:59 PM"
Preprocessor: "IfcOpenShell 0.5.0-dev"
Originating system: "IfcOpenShell 0.5.0-dev"
Application: "Klemen" version "v1.0" by Organization (no name given)

People and organizations
  Person (no name given) of Organization (no name given)
  Owner history of Person (no name given) of Organization (no name given) | application "Klemen" version "v1.0" by Organization (no name given) | change ADDED | created 1636095297 (2021-11-05T06:54:57Z) | last modified by Person (no name given) of Organization (no name given) with "Klemen" version "v1.0" by Organization (no name given)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)

Spatial structure
IFCPROJECT "001101028"
  IFCSITE "Default Site"
    IFCBUILDING "Default Building"
      IFCBUILDINGSTOREY "Default Storey"
        contains 135 elements
          135 x IFCBUILDINGELEMENTPROXY | names: "YZ_Plane002", "X_Axis005", "Y_Axis005" (+132 more) | property sets: Basic product data:, Dimensions:, Technical data:, Logistic data:, Manufacturer data:, Contacts:

Property sets
  Basic product data: | properties | on 148 objects (135 IFCBUILDINGELEMENTPROXY, 13 (other))
    Code: = "001101028" (IFCTEXT)
    Name: = "ECG56" (IFCTEXT)
    Product group: = "ETIBOX Distribution boards, metal enclosures and free-standing cable distribution cabinets" (IFCTEXT)
    Product link: = "https://www.etigroup.eu/products-services/001101028" (IFCTEXT)
    Short description: = "Distribution box, ECG56" (IFCTEXT)
  Dimensions: | properties | on 148 objects (135 IFCBUILDINGELEMENTPROXY, 13 (other))
    Depth (mm): = "87" (IFCTEXT)
    Height (mm): = "717" (IFCTEXT)
    Width (mm): = "346" (IFCTEXT)
  Technical data: | properties | on 148 objects (135 IFCBUILDINGELEMENTPROXY, 13 (other))
    Frequency (Hz): = "/" (IFCTEXT)
    Fusing characteristics: = "/" (IFCTEXT)
    IP Rating: = "IP40" (IFCTEXT)
    Number of poles: = "/" (IFCTEXT)
    Power dissipation (W): = "/" (IFCTEXT)
    Rated current (A): = "63" (IFCTEXT)
    Rated voltage AC (V): = "400" (IFCTEXT)
    Rated voltage DC (V): = "400" (IFCTEXT)
    Voltage type: = "AC/DC" (IFCTEXT)
    Weight (kg): = "3.5" (IFCTEXT)
  Logistic data: | properties | on 148 objects (135 IFCBUILDINGELEMENTPROXY, 13 (other))
    Basic packaging: = "1" (IFCTEXT)
    EAN (single product): = "3838895689690" (IFCTEXT)
  Manufacturer data: | properties | on 148 objects (135 IFCBUILDINGELEMENTPROXY, 13 (other))
    City: = "Izlake" (IFCTEXT)
    Country: = "Slovenia" (IFCTEXT)
    Manufacturer: = "ETI Elektroelement d.o.o." (IFCTEXT)
    Postal code: = "1411" (IFCTEXT)
    Street: = "Obrezija 5" (IFCTEXT)
    Website: = "https://www.etigroup.eu/" (IFCTEXT)
  Contacts: | properties | on 148 objects (135 IFCBUILDINGELEMENTPROXY, 13 (other))
    E-mail: = "support@eti.si" (IFCTEXT)
    Fax: = "00386 (0)3 / 56-74-077" (IFCTEXT)
    Telephone: = "00386 (0)3 / 56-57-570" (IFCTEXT)
  ETIM Classification v7.0: | properties | on 148 objects (135 IFCBUILDINGELEMENTPROXY, 13 (other))
    Built-in depth (mm): = "88" (IFCTEXT)
    Class name: = "Small distribution board" (IFCTEXT)
    Classification: = "EC000214" (IFCTEXT)
    Colour: = "White" (IFCTEXT)
    DIN-rail: = "True" (IFCTEXT)
    Degree of protection (IP): = "IP40" (IFCTEXT)
    Depth (mm): = "87" (IFCTEXT)
    EMC-version: = "True" (IFCTEXT)
    Height (mm): = "717" (IFCTEXT)
    Material housing: = "Plastic" (IFCTEXT)
    Mounting method: = "Flush mounted (plaster)" (IFCTEXT)
    Number of rows: = "4" (IFCTEXT)
    Width (mm): = "346" (IFCTEXT)
    Width in number of modular spacings: = "14" (IFCTEXT)
    With mounting plate: = "False" (IFCTEXT)