IFC building model
Schema: "IFC2X3"
File name: "Sample.ifc"
Time stamp: "12/11/2021 2:47:18 PM"
Preprocessor: "IfcOpenShell 0.5.0-dev"
Originating system: "IfcOpenShell 0.5.0-dev"
Application: "Klemen" version "v1.0" by Organization (no name given)

People and organizations
  Person (no name given) of Organization (no name given)
  Owner history of Person (no name given) of Organization (no name given) | application "Klemen" version "v1.0" by Organization (no name given) | change ADDED | created 1636033175 (2021-11-04T13:39:35Z) | last modified by Person (no name given) of Organization (no name given) with "Klemen" version "v1.0" by Organization (no name given)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)

Spatial structure
IFCPROJECT "001100243"
  IFCSITE "Default Site"
    IFCBUILDING "Default Building"
      IFCBUILDINGSTOREY "Default Storey"
        contains 21 elements
          21 x IFCBUILDINGELEMENTPROXY | names: "PLASTICNI_SRAF_MASKE_TEHNOPLAST002", "PLASTICNI_SRAF_MASKE_TEHNOPLAST003", "DNO_12_ALFA__12_04_2018___1_1" (+18 more) | property sets: Basic product data:, Dimensions:, Technical data:, Logistic data:, Manufacturer data:, Contacts:

Property sets
  Basic product data: | properties | on 38 objects (21 IFCBUILDINGELEMENTPROXY, 17 (other))
    Code: = "001100243" (IFCTEXT)
    Name: = "ACT12PO" (IFCTEXT)
    Product group: = "ETIBOX Distribution boards, metal enclosures and free-standing cable distribution cabinets" (IFCTEXT)
    Product link: = "https://www.etigroup.eu/products-services/001100243" (IFCTEXT)
    Short description: = "Distribution box, ACT12PO" (IFCTEXT)
  Dimensions: | properties | on 38 objects (21 IFCBUILDINGELEMENTPROXY, 17 (other))
    Depth (mm): = "96" (IFCTEXT)
    Height (mm): = "251" (IFCTEXT)
    Width (mm): = "310" (IFCTEXT)
  Technical data: | properties | on 38 objects (21 IFCBUILDINGELEMENTPROXY, 17 (other))
    Frequency (Hz): = "/" (IFCTEXT)
    Fusing characteristics: = "/" (IFCTEXT)
    IP Rating: = "IP40" (IFCTEXT)
    Number of poles: = "/" (IFCTEXT)
    Power dissipation (W): = "/" (IFCTEXT)
    Rated current (A): = "/" (IFCTEXT)
    Rated voltage AC (V): = "400" (IFCTEXT)
    Rated voltage DC (V): = "400" (IFCTEXT)
    Voltage type: = "AC/DC" (IFCTEXT)
    Weight (kg): = "1.2" (IFCTEXT)
  Logistic data: | properties | on 38 objects (21 IFCBUILDINGELEMENTPROXY, 17 (other))
    Basic packaging: = "1" (IFCTEXT)
    EAN (single product): = "3838895838739" (IFCTEXT)
  Manufacturer data: | properties | on 38 objects (21 IFCBUILDINGELEMENTPROXY, 17 (other))
    City: = "Izlake" (IFCTEXT)
    Country: = "Slovenia" (IFCTEXT)
    Manufacturer: = "ETI Elektroelement d.o.o." (IFCTEXT)
    Postal code: = "1411" (IFCTEXT)
    Street: = "Obrezija 5" (IFCTEXT)
    Website: = "https://www.etigroup.eu/" (IFCTEXT)
  Contacts: | properties | on 38 objects (21 IFCBUILDINGELEMENTPROXY, 17 (other))
    E-mail: = "support@eti.si" (IFCTEXT)
    Fax: = "00386 (0)3 / 56-74-077" (IFCTEXT)
    Telephone: = "00386 (0)3 / 56-57-570" (IFCTEXT)
  ETIM Classification v7.0: | properties | on 38 objects (21 IFCBUILDINGELEMENTPROXY, 17 (other))
    Class name: = "Small distribution board" (IFCTEXT)
    Classification: = "EC000214" (IFCTEXT)
    Colour: = "White" (IFCTEXT)
    DIN-rail: = "True" (IFCTEXT)
    Degree of protection (IP): = "IP40" (IFCTEXT)
    Depth (mm): = "96" (IFCTEXT)
    EMC-version: = "True" (IFCTEXT)
    Height (mm): = "251" (IFCTEXT)
    Material housing: = "Plastic" (IFCTEXT)
    Mounting method: = "Surface mounting" (IFCTEXT)
    Number of rows: = "1" (IFCTEXT)
    RAL-number: = "9003" (IFCTEXT)
    Width (mm): = "310" (IFCTEXT)
    Width in number of modular spacings: = "14" (IFCTEXT)
    With mounting plate: = "False" (IFCTEXT)