IFC building model
Schema: "IFC2X3"
File name: "Sample.ifc"
Time stamp: "12/11/2021 2:53:30 PM"
Preprocessor: "IfcOpenShell 0.5.0-dev"
Originating system: "IfcOpenShell 0.5.0-dev"
Application: "Klemen" version "v1.0" by Organization (no name given)

People and organizations
  Person (no name given) of Organization (no name given)
  Owner history of Person (no name given) of Organization (no name given) | application "Klemen" version "v1.0" by Organization (no name given) | change ADDED | created 1636097861 (2021-11-05T07:37:41Z) | last modified by Person (no name given) of Organization (no name given) with "Klemen" version "v1.0" by Organization (no name given)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)

Spatial structure
IFCPROJECT "001101169"
  IFCSITE "Default Site"
    IFCBUILDING "Default Building"
      IFCBUILDINGSTOREY "Default Storey"
        contains 182 elements
          182 x IFCBUILDINGELEMENTPROXY | names: "BPA002", "X_Axis", "Y_Axis" (+179 more) | property sets: Basic product data:, Dimensions:, Technical data:, Logistic data:, Manufacturer data:, Contacts:

Property sets
  Basic product data: | properties | on 182 objects (182 IFCBUILDINGELEMENTPROXY)
    Code: = "001101169" (IFCTEXT)
    Name: = "ECG70H" (IFCTEXT)
    Product group: = "ETIBOX Distribution boards, metal enclosures and free-standing cable distribution cabinets" (IFCTEXT)
    Product link: = "https://www.etigroup.eu/products-services/001101169" (IFCTEXT)
    Short description: = "Distribution box, ECG70H" (IFCTEXT)
  Dimensions: | properties | on 182 objects (182 IFCBUILDINGELEMENTPROXY)
    Depth (mm): = "425" (IFCTEXT)
    Height (mm): = "842" (IFCTEXT)
    Width (mm): = "95" (IFCTEXT)
  Technical data: | properties | on 182 objects (182 IFCBUILDINGELEMENTPROXY)
    Frequency (Hz): = "/" (IFCTEXT)
    Fusing characteristics: = "/" (IFCTEXT)
    IP Rating: = "IP40" (IFCTEXT)
    Number of poles: = "/" (IFCTEXT)
    Power dissipation (W): = "/" (IFCTEXT)
    Rated current (A): = "63" (IFCTEXT)
    Rated voltage AC (V): = "400" (IFCTEXT)
    Rated voltage DC (V): = "400" (IFCTEXT)
    Voltage type: = "AC/DC" (IFCTEXT)
    Weight (kg): = "5" (IFCTEXT)
  Logistic data: | properties | on 182 objects (182 IFCBUILDINGELEMENTPROXY)
    Basic packaging: = "1" (IFCTEXT)
    EAN (single product): = "3838895821656" (IFCTEXT)
  Manufacturer data: | properties | on 182 objects (182 IFCBUILDINGELEMENTPROXY)
    City: = "Izlake" (IFCTEXT)
    Country: = "Slovenia" (IFCTEXT)
    Manufacturer: = "ETI Elektroelement d.o.o." (IFCTEXT)
    Postal code: = "1411" (IFCTEXT)
    Street: = "Obrezija 5" (IFCTEXT)
    Website: = "https://www.etigroup.eu/" (IFCTEXT)
  Contacts: | properties | on 182 objects (182 IFCBUILDINGELEMENTPROXY)
    E-mail: = "support@eti.si" (IFCTEXT)
    Fax: = "00386 (0)3 / 56-74-077" (IFCTEXT)
    Telephone: = "00386 (0)3 / 56-57-570" (IFCTEXT)
  ETIM Classification v7.0: | properties | on 182 objects (182 IFCBUILDINGELEMENTPROXY)
    Class name: = "Small distribution board" (IFCTEXT)
    Classification: = "EC000214" (IFCTEXT)
    Colour: = "Other" (IFCTEXT)
    Degree of protection (IP): = "Other" (IFCTEXT)
    Mounting method: = "Other" (IFCTEXT)